**Specifikimet Teknike**

Caritas Shqiptar kerkon blerjen e pajisjeve elektronike si meposhte vijon:

1. **Kompjuter Desktop me specifikat e meposhtme:**

Modeli 1

* Procesori (CPU): ≥ Intel Core i5-8400 4.00 GHz
* Memorja (RAM): ≥ 12GB DDR4-2666MHz
* Hard Disku (HDD): ≥ 256 GB SSD
* ODD: DVD +/- RW SuperMulti DL
* Karta Grafike (VGA): ≥ Intel HD
* Sistemi Operativ (OS): Windows 10 Licensed
* Keyboard: QWERTY Keyboard, English Layout
* Mouse: Optical, 1000 DPI sensitivity

Modeli 2

* Procesori (CPU): ≥ Intel Core i3-8100 3.6 GHz
* Memorja (RAM): ≥ 8GB DDR4-2666MHz
* Hard Disku (HDD): ≥ 256 GB SSD
* ODD: DVD +/- RW SuperMulti DL
* Karta Grafike (VGA): ≥ Intel HD
* Sistemi Operativ (OS): Free DOS
* Keyboard: QWERTY Keyboard, English Layout
* Mouse: Optical, 1000 DPI sensitivity
1. **Monitor Kompjuteri me specifikat e meposhtme:**
* Size: 23.8 inch
* Resolution: 1920 x 1080 pixels, Full HD/1080p
* Connectivity: 1xHDMI 1.4, 1x DispalyPort 1.2, 1 x D-Sub
* Accessories: D-Sub Cable, DisplayPort Cable, HDMI Cable
1. **Laptop me specifikat e meposhtme:**

Modeli 1

* Procesori (CPU): ≥ Intel Core i5 7th Gen
* Memorja (RAM): ≥ 8GB DDR4
* Hard Disk (HDD): ≥ 128 GB SSD
* ODD: DVD +/- RW SuperMulti DL
* Sistemi Operativ: Free DOS
* Ekran: 15,6” (1920 x 1080)
* Portat: ≥
	+ (3) USB,
	+ (1) HDMI,
	+ (1) VGA,
	+ (1) Ethernet,
	+ (1) Headphone/microphone combo jack

Modeli 2

* Procesori (CPU): ≥ Intel Core i7 7th Gen
* Memorja (RAM): ≥ 16GB DDR4
* Hard Disk (HDD): ≥ 256 GB SSD
* ODD: DVD +/- RW SuperMulti DL
* Sistemi Operativ: Windows 10 Licensed
* Ekran: 15,6” (1920 x 1080)
* Portat: ≥
	+ (3) USB,
	+ (1) HDMI,
	+ (1) VGA,
	+ (1) Ethernet,
	+ (1) Headphone/microphone combo jack
1. **Projektor me specifikat e meposhtme:**
* IMAGE DISPLAY
	+ - * NATIVE RESOLUTION: 800 x 600
			* MAXIMUM RESOLUTION: 1920 x 1200
* LENS
* MAXIMUM PROJECTION DISTANCE: 11.80 m
* LAMP
* NUMBER OF LAMPS: 1
* NORMAL MODE LAMP LIFE: 6000 Hour
* INTERFACES / PORTS
* 1 x HDMI
* 1 x USB
* 1 x VGA in
* 1 x VGA out
* 1 x Audio in
* 1 x Audio out
1. **Aparat Profesional me specifikat e meposhtme:**

Modeli 1

* Camera with 18-140mm Lens
* 20.9MP DX-Format CMOS Sensor
* EXPEED 5 Image Processor
* 3.2" 922k-Dot Tilting Touchscreen LCD
* 4K UHD Video Recording at 30 fps
* Multi-CAM 3500FX II 51-Point AF System
* Native ISO 51200, Expanded ISO 1,640,000
* 8 fps Shooting for Up to 100 Frames
* SnapBridge Bluetooth and Wi-Fi
* 180k-Pixel RGB Sensor and Group Area AF
* AF-S DX 18-140mm f/3.5-5.6G ED VR Len

Modeli 2

* Compatible memory cards: SD, SDHC, SDXC
* Memory slots: 1
* Maximum video resolution: 1920 x 1080 pixels
* Full HD: Y
* Video formats supported: H.264
* Video resolutions: 640 x 480, 1280 x 720, 1920 x 1080 pixels
* Analog signal format system: NTSC, PAL
* Motion JPEG frame rate : 29.97 fps
* Colour of product: Black
* Self-timer: 2, 10s
* Camera playback: Movie, Single image, Slide show
* Viewfinder type: Electrical
* Light exposure control: Program AE
* Built-in flash: Y
* PictBridge: Y
* HDMI: Y
* USB version: 2.0
* HDMI connector type: Mini
* Microphone in: Y
* Battery technology: Lithium-Ion (Li-Ion)
* Battery type: LP-E8
* Number of batteries supported: 1
* Display: TFT
* Display resolution (numeric): 1040000 pixels
* Field of view: 100%
* Vari-angle LCD display: Y
* Touch screen: Y
* Display diagonal: 7.62 cm (3")
* Lens structure (elements/groups): 13-nov
* Filter size: 5.8 cm
* Lens mount interface: Canon EF, Canon EF-S
* Focal length range (f-f): 18 - 55 mm
* Minimum focal length (35mm film equiv): 2.9 cm
* Maximum focal length (35mm film equiv): 8.8 cm
* Minimum aperture number: 3.5
* Maximum aperture number: 38
* Number of diaphragm blades: 7
* Camera type: SLR Camera Kit
* White balance: Auto, Cloudy, Daylight, Flash, Fluorescent L, Shade, Tungsten
* Scene modes: Close-up (macro), Landscape, Night, Night portrait, Portrait, Sports
* Shooting modes Aperture priority, Auto, Manual, Movie, Program, Scene, Shutter Playback zoom (max)
* Camera file system: DCF 2.0, DPOF 1.1, Exif 2.3, RAW
* Dioptre correction: Y
* Histogram: Y
* Live view: Y
* Built-in processor: DIGIC 5
* Auto focusing (AF) modes: Continuous Auto Focus, Servo Auto Focus, Single Auto Focus
* Focus: TTL
* Focus adjustment: Auto/Manual
* Closest focusing distance: 0.25m
* ISO sensitivity: 100, 200, 400, 800, 1600, 3200, 6400, 12800, Auto
* Light exposure modes: Aperture priority AE, Auto, Manual, Shutter priority AE
* Light exposure correction: ± 5EV (1/3EV step)
* Light metering: Centre-weighted, Evaluative (Multi-pattern), Spot
* Auto Exposure (AE) lock: Y
* ISO sensitivity (max): 12800
* ISO sensitivity (min): 100
* Flash modes: Auto, Manual, Red-eye reduction
* Flash exposure compensation: Y
* Flash exposure correction: ±2EV (1/2, 1/3 EV step)
* Flash exposure lock: Y
* Flash sync-speed: 1/200s